|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Fluid Resistant Respirators**  Note: the addition of a face shield may increase fluid protection | | | | |
| **Mask image** | **Details** | **Applicable Standards** | **Protection levels** | **Other** |
|  | **3M: 1860**  N95  Size: medium  Box 20 | NIOSH 42, CFR Part 84 | PFE >95%  BFE >99%  FRL: 2 (120mmHg) | ARTG: 255656  NIOSH TC-84A-0006 |
| 3M™ Particulate Healthcare Respirator, 1860S, N95, 120 per case | **3M: 1860S**  N95  Size: small  Box 20 | NIOSH 42, CFR Part 84 | PFE >95%  BFE >99%  FRL: 1 (80mmHg) | ARTG: 255656  NIOSH TC-84A-0006 |
|  | **BSN: 72509-09**  N95  Size: small  Box 50 | NIOSH 42, CFR Part 84 | PFR >95%  BFE ≥ 98%  FRL: 3 (160mmHg) | ARTG: 305431  NIOSH TC-84A-3348 |
|  | **BSN: 72509-10**  N95  Size: medium  Box 50 | NIOSH 42, CFR Part 84  AS/NZ 1716:2012 | PFE >95%  FRL: 3 (160mmHg) | ARTG: 334581  NIOSH TC-84A-3348 |
|  | **BYD: DE2322**  N95  Size: medium  Box 25 | NIOSH 42, CFR Part 84  AS 4381:2015  GB 19083-2010  ASTM F2100 | PFE >95%  BFE > 99%  FRL: 3 (160mmHg) | ARTG:337767  Note: 332300 superseded in June 2020  NIOSH TC-84A-9221 |
|  | **Everyday Office National (Honeywell): H910 Plus series, part number #SP910**  N95  Size: regular  Box 50 | NIOSH 42, CFR Part 84  EN14683:2014  EN14683:2019 | PFE >95%  BFE >98%  FRL: IIR (120mmHg) | ARTG: 335988  NIOSH TC- 84A-8480 |
|  | **AlphaProTech: 695**  N95  Size: universal  Box 35 | NIOSH 42, CFR Part 84  ASTM F2100 | PFE ≥ 98%  BFE ≥ 98%  FRL: 3 (160mmHg) | ARTG: 331773  NIOSH TC-84A-0457 |
|  | **3M: 9320A+**  P2  Size: regular  Case 400 | AS/NZS 1716:2012  AS/NZS 4381:2015  AS4381:2015 | PFE ≥ 94%  FRL: 2 (120mmHg) | ARTG:335620  BSI: BMP 572181 -(compliance to AS/NZS 1716:2012) |
|  | **O&M Halyard: 46727**  N95  Size: standard  Box 35 | NIOSH 42, CFR Part 84  ASTM F2100-11 | PFE ≥ 98%  BFE ≥ 98%  FRL: 3 (160mmHg) | ARTG: 314855  NIOSH TC-84A-7521 |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Non-fluid resistant Respirators**  Note: the addition of a faceshield may increase fluid protection | | | | |
| **Mask image** | **Details** | **Applicable Standards** | **Protection levels** | **Other** |
| 3M Particulate Respirator (Mask) 8210, N95 - Adore Pharmacy | **3M: 8210**  P2/N95  Size: medium  Box 20 | NIOSH 42, CFR Part 84  AS/NZ 1716:2012 | PFE >95%  FRL: Nil | ARTG: 334581  NIOSH TC-84A-0007  SAI Global Standards Mark License: SMKH20654 |
| 3M(TM)  Particulate Respirator 8110S, N95 | **3M: 8110S**  P2/N95  Size: small  Box 20 | NIOSH 42, CFR Part 84 | PFE >95%  FRL: Nil | ARTG: 33458  NIOSH TC-84A-0007 |
|  | **Detmold: W376**  P2  Size: medium  Box 25  Comes with small ear saver clip | AS/NZ 1716:2012  AS 4381: 2015  ASTM F2100  EN 14683:2019 | BFE ≥ 98%  FRL: Nil claimed | ARTG: 337768 |
| **Ear saver buckles/clips (may improve fit of ear loop mask)** | | | | |
| **Roo Technologies**  **RT-0005-02**  Box 20 |  |  | **VB Precision Tooling**  **B-1963**  Box 500 |  |
| **Detmold Fit Clip XL**  **W008S0001**  69mm x 19mm  Box 50 |  |  |  |  |